4/2/16

Shading tests for 2016.3.14 Pi Patch 1 – test SWH, PVWatts and PV with mxh, timeseries, and Sun Eye import and store project files for future tests and results stored in

C:\Projects\SAM\Documentation\SAMnt\testing\Shading

Annual energy

PVWatts – no shading 6830

PVWatts – 3d scene 5434

PVWatts – SunEye Sky02 6428

PVWatts – SunEye old 6297

Annual energy saved

SWH – no shading 2106

SWH – 3d scene 1750

SWH – SunEye Sky02 2083

SWH – SunEye old 2016

Annual energy

PV – no shading 7408

PV – 3d scene 5821

PV – SunEye Sky02 7007

PV – SunEye old 6847